Next: PDP-11 Options, Previous: Nvidia PTX Options, Up: Submodel Options [Contents][Index]

#### 3.19.37 OpenRISC Options

These options are defined for OpenRISC:

`-mboard=name`

  Configure a board specific runtime. This will be passed to the linker for newlib board library linking. The default is `or1ksim`.

`-mnewlib`

  This option is ignored; it is for compatibility purposes only. This used to select linker and preprocessor options for use with newlib.

`-msoft-div`
`-mhard-div`

  Select software or hardware divide (`l.div`, `l.divu`) instructions. This default is hardware divide.

`-msoft-mul`
`-mhard-mul`

  Select software or hardware multiply (`l.mul`, `l.muli`) instructions. This default is hardware multiply.

`-msoft-float`
`-mhard-float`

  Select software or hardware for floating point operations. The default is software.

`-mdouble-float`

  When `-mhard-float` is selected, enables generation of double-precision floating point instructions. By default functions from `libgcc` are used to perform double-precision floating point operations.

`-munordered-float`

  When `-mhard-float` is selected, enables generation of unordered floating point compare and set flag (`lf.sfun*`) instructions. By default functions from `libgcc` are used to perform unordered floating point compare and set flag operations.

`-mcmov`

  Enable generation of conditional move (`l.cmov`) instructions. By default the equivalent will be generated using set and branch.

`-mror`

  Enable generation of rotate right (`l.ror`) instructions. By default functions from `libgcc` are used to perform rotate right operations.

`-mrori`

  Enable generation of rotate right with immediate (`l.rori`) instructions. By default functions from `libgcc` are used to perform rotate right with immediate operations.

`-msext`

  Enable generation of sign extension (`l.ext*`) instructions. By default memory loads are used to perform sign extension.

`-msfimm`

  Enable generation of compare and set flag with immediate (`l.sf*i`) instructions. By default extra instructions will be generated to store the immediate to a register first.

`-mshftimm`

  Enable generation of shift with immediate (`l.srai`, `l.srli`, `l.slli`) instructions. By default extra instructions will be generated to store the immediate to a register first.

Next: PDP-11 Options, Previous: Nvidia PTX Options, Up: Submodel Options [Contents][Index]