Next: picoChip Options, Previous: OpenRISC Options, Up: Submodel Options [Contents][Index]

#### 3.19.38 PDP-11 Options

These options are defined for the PDP-11:

`-mfpu`

  Use hardware FPP floating point. This is the default. (FIS floating point on the PDP-11/40 is not supported.) Implies -m45.

`-msoft-float`

  Do not use hardware floating point.

`-mac0`

  Return floating-point results in ac0 (fr0 in Unix assembler syntax).

`-mno-ac0`

  Return floating-point results in memory. This is the default.

`-m40`

  Generate code for a PDP-11/40. Implies -msoft-float -mno-split.

`-m45`

  Generate code for a PDP-11/45. This is the default.

`-m10`

  Generate code for a PDP-11/10. Implies -msoft-float -mno-split.

`-mint16`
`-mno-int32`

  Use 16-bit `int`. This is the default.

`-mint32`
`-mno-int16`

  Use 32-bit `int`.

`-msplit`

  Target has split instruction and data space. Implies -m45.

`-munix-asm`

  Use Unix assembler syntax.

`-mdec-asm`

  Use DEC assembler syntax.

`-mgnu-asm`

  Use GNU assembler syntax. This is the default.

`-mlra`

  Use the new LRA register allocator. By default, the old “reload” allocator is used.