Next: AVR Built-in Functions, Previous: ARM Floating Point Status and Control Intrinsics, Up: Target Builtins [Contents][Index]

#### 6.60.9 ARM ARMv8-M Security Extensions

GCC implements the ARMv8-M Security Extensions as described in the ARMv8-M Security Extensions: Requirements on Development Tools Engineering Specification, which can be found at https://developer.arm.com/documentation/ecm0359818/latest/.

As part of the Security Extensions GCC implements two new function attributes: `cmse_nonsecure_entry` and `cmse_nonsecure_call`.

As part of the Security Extensions GCC implements the intrinsics below. FPTR is used here to mean any function pointer type.

    cmse_address_info_t cmse_TT (void *)
    cmse_address_info_t cmse_TT_fptr (FPTR)
    cmse_address_info_t cmse_TTT (void *)
    cmse_address_info_t cmse_TTT_fptr (FPTR)
    cmse_address_info_t cmse_TTA (void *)
    cmse_address_info_t cmse_TTA_fptr (FPTR)
    cmse_address_info_t cmse_TTAT (void *)
    cmse_address_info_t cmse_TTAT_fptr (FPTR)
    void * cmse_check_address_range (void *, size_t, int)
    typeof(p) cmse_nsfptr_create (FPTR p)
    intptr_t cmse_is_nsfptr (FPTR)
    int cmse_nonsecure_caller (void)