Next: Scalar Return, Previous: Stack Arguments, Up: Stack and Calling [Contents][Index]

#### 18.9.7 Passing Arguments in Registers

This section describes the macros which let you control how various types of arguments are passed in registers or how they are arranged in the stack.

Target Hook: rtx TARGET_FUNCTION_ARG (cumulative_args_t ca, const function_arg_info &arg)

  Return an RTX indicating whether function argument arg is passed in a register and if so, which register. Argument ca summarizes all the previous arguments.

  The return value is usually either a `reg` RTX for the hard register in which to pass the argument, or zero to pass the argument on the stack.

  The return value can be a `const_int` which means argument is passed in a target specific slot with specified number. Target hooks should be used to store or load argument in such case. See `TARGET_STORE_BOUNDS_FOR_ARG` and `TARGET_LOAD_BOUNDS_FOR_ARG` for more information.

  The value of the expression can also be a `parallel` RTX. This is used when an argument is passed in multiple locations. The mode of the `parallel` should be the mode of the entire argument. The `parallel` holds any number of `expr_list` pairs; each one describes where part of the argument is passed. In each `expr_list` the first operand must be a `reg` RTX for the hard register in which to pass this part of the argument, and the mode of the register RTX indicates how large this part of the argument is. The second operand of the `expr_list` is a `const_int` which gives the offset in bytes into the entire argument of where this part starts. As a special exception the first `expr_list` in the `parallel` RTX may have a first operand of zero. This indicates that the entire argument is also stored on the stack.

  The last time this hook is called, it is called with `MODE == VOIDmode`, and its result is passed to the `call` or `call_value` pattern as operands 2 and 3 respectively.

  The usual way to make the ISO library `stdarg.h` work on a machine where some arguments are usually passed in registers, is to cause nameless arguments to be passed on the stack instead. This is done by making `TARGET_FUNCTION_ARG` return 0 whenever named is `false`.

  You may use the hook `targetm.calls.must_pass_in_stack` in the definition of this macro to determine if this argument is of a type that must be passed in the stack. If `REG_PARM_STACK_SPACE` is not defined and `TARGET_FUNCTION_ARG` returns nonzero for such an argument, the compiler will abort. If `REG_PARM_STACK_SPACE` is defined, the argument will be computed in the stack and then loaded into a register.

Target Hook: bool TARGET_MUST_PASS_IN_STACK (const function_arg_info &arg)

  This target hook should return `true` if we should not pass arg solely in registers. The file `expr.h` defines a definition that is usually appropriate, refer to `expr.h` for additional documentation.

Target Hook: rtx TARGET_FUNCTION_INCOMING_ARG (cumulative_args_t ca, const function_arg_info &arg)

  Define this hook if the caller and callee on the target have different views of where arguments are passed. Also define this hook if there are functions that are never directly called, but are invoked by the hardware and which have nonstandard calling conventions.

  In this case `TARGET_FUNCTION_ARG` computes the register in which the caller passes the value, and `TARGET_FUNCTION_INCOMING_ARG` should be defined in a similar fashion to tell the function being called where the arguments will arrive.

  `TARGET_FUNCTION_INCOMING_ARG` can also return arbitrary address computation using hard register, which can be forced into a register, so that it can be used to pass special arguments.

  If `TARGET_FUNCTION_INCOMING_ARG` is not defined, `TARGET_FUNCTION_ARG` serves both purposes.

Target Hook: bool TARGET_USE_PSEUDO_PIC_REG (void)

  This hook should return 1 in case pseudo register should be created for pic_offset_table_rtx during function expand.

Target Hook: void TARGET_INIT_PIC_REG (void)

  Perform a target dependent initialization of pic_offset_table_rtx. This hook is called at the start of register allocation.

Target Hook: int TARGET_ARG_PARTIAL_BYTES (cumulative_args_t cum, const function_arg_info &arg)

  This target hook returns the number of bytes at the beginning of an argument that must be put in registers. The value must be zero for arguments that are passed entirely in registers or that are entirely pushed on the stack.

  On some machines, certain arguments must be passed partially in registers and partially in memory. On these machines, typically the first few words of arguments are passed in registers, and the rest on the stack. If a multi-word argument (a `double` or a structure) crosses that boundary, its first few words must be passed in registers and the rest must be pushed. This macro tells the compiler when this occurs, and how many bytes should go in registers.

  `TARGET_FUNCTION_ARG` for these arguments should return the first register to be used by the caller for this argument; likewise `TARGET_FUNCTION_INCOMING_ARG`, for the called function.

Target Hook: bool TARGET_PASS_BY_REFERENCE (cumulative_args_t cum, const function_arg_info &arg)

  This target hook should return `true` if argument arg at the position indicated by cum should be passed by reference. This predicate is queried after target independent reasons for being passed by reference, such as `TREE_ADDRESSABLE (arg.type)`.

  If the hook returns true, a copy of that argument is made in memory and a pointer to the argument is passed instead of the argument itself. The pointer is passed in whatever way is appropriate for passing a pointer to that type.

Target Hook: bool TARGET_CALLEE_COPIES (cumulative_args_t cum, const function_arg_info &arg)

  The function argument described by the parameters to this hook is known to be passed by reference. The hook should return true if the function argument should be copied by the callee instead of copied by the caller.

  For any argument for which the hook returns true, if it can be determined that the argument is not modified, then a copy need not be generated.

  The default version of this hook always returns false.

Macro: CUMULATIVE_ARGS

  A C type for declaring a variable that is used as the first argument of `TARGET_FUNCTION_ARG` and other related values. For some target machines, the type `int` suffices and can hold the number of bytes of argument so far.

  There is no need to record in `CUMULATIVE_ARGS` anything about the arguments that have been passed on the stack. The compiler has other variables to keep track of that. For target machines on which all arguments are passed on the stack, there is no need to store anything in `CUMULATIVE_ARGS`; however, the data structure must exist and should not be empty, so use `int`.

Macro: OVERRIDE_ABI_FORMAT (fndecl)

  If defined, this macro is called before generating any code for a function, but after the cfun descriptor for the function has been created. The back end may use this macro to update cfun to reflect an ABI other than that which would normally be used by default. If the compiler is generating code for a compiler-generated function, fndecl may be `NULL`.

Macro: INIT_CUMULATIVE_ARGS (cum, fntype, libname, fndecl, n_named_args)

  A C statement (sans semicolon) for initializing the variable cum for the state at the beginning of the argument list. The variable has type `CUMULATIVE_ARGS`. The value of fntype is the tree node for the data type of the function which will receive the args, or 0 if the args are to a compiler support library function. For direct calls that are not libcalls, fndecl contain the declaration node of the function. fndecl is also set when `INIT_CUMULATIVE_ARGS` is used to find arguments for the function being compiled. n_named_args is set to the number of named arguments, including a structure return address if it is passed as a parameter, when making a call. When processing incoming arguments, n_named_args is set to -1.

  When processing a call to a compiler support library function, libname identifies which one. It is a `symbol_ref` rtx which contains the name of the function, as a string. libname is 0 when an ordinary C function call is being processed. Thus, each time this macro is called, either libname or fntype is nonzero, but never both of them at once.

Macro: INIT_CUMULATIVE_LIBCALL_ARGS (cum, mode, libname)

  Like `INIT_CUMULATIVE_ARGS` but only used for outgoing libcalls, it gets a `MODE` argument instead of fntype, that would be `NULL`. indirect would always be zero, too. If this macro is not defined, `INIT_CUMULATIVE_ARGS (cum, NULL_RTX, libname, 0)` is used instead.

Macro: INIT_CUMULATIVE_INCOMING_ARGS (cum, fntype, libname)

  Like `INIT_CUMULATIVE_ARGS` but overrides it for the purposes of finding the arguments for the function being compiled. If this macro is undefined, `INIT_CUMULATIVE_ARGS` is used instead.

  The value passed for libname is always 0, since library routines with special calling conventions are never compiled with GCC. The argument libname exists for symmetry with `INIT_CUMULATIVE_ARGS`.

Target Hook: void TARGET_FUNCTION_ARG_ADVANCE (cumulative_args_t ca, const function_arg_info &arg)

  This hook updates the summarizer variable pointed to by ca to advance past argument arg in the argument list. Once this is done, the variable cum is suitable for analyzing the following argument with `TARGET_FUNCTION_ARG`, etc.

  This hook need not do anything if the argument in question was passed on the stack. The compiler knows how to track the amount of stack space used for arguments without any special help.

Target Hook: HOST_WIDE_INT TARGET_FUNCTION_ARG_OFFSET (machine_mode mode, const_tree type)

  This hook returns the number of bytes to add to the offset of an argument of type type and mode mode when passed in memory. This is needed for the SPU, which passes `char` and `short` arguments in the preferred slot that is in the middle of the quad word instead of starting at the top. The default implementation returns 0.

Target Hook: pad_direction TARGET_FUNCTION_ARG_PADDING (machine_mode mode, const_tree type)

  This hook determines whether, and in which direction, to pad out an argument of mode mode and type type. It returns `PAD_UPWARD` to insert padding above the argument, `PAD_DOWNWARD` to insert padding below the argument, or `PAD_NONE` to inhibit padding.

  The amount of padding is not controlled by this hook, but by `TARGET_FUNCTION_ARG_ROUND_BOUNDARY`. It is always just enough to reach the next multiple of that boundary.

  This hook has a default definition that is right for most systems. For little-endian machines, the default is to pad upward. For big-endian machines, the default is to pad downward for an argument of constant size shorter than an `int`, and upward otherwise.

Macro: PAD_VARARGS_DOWN

  If defined, a C expression which determines whether the default implementation of va_arg will attempt to pad down before reading the next argument, if that argument is smaller than its aligned space as controlled by `PARM_BOUNDARY`. If this macro is not defined, all such arguments are padded down if `BYTES_BIG_ENDIAN` is true.

Macro: BLOCK_REG_PADDING (mode, type, first)

  Specify padding for the last element of a block move between registers and memory. first is nonzero if this is the only element. Defining this macro allows better control of register function parameters on big-endian machines, without using `PARALLEL` rtl. In particular, `MUST_PASS_IN_STACK` need not test padding and mode of types in registers, as there is no longer a "wrong" part of a register; For example, a three byte aggregate may be passed in the high part of a register if so required.

Target Hook: unsigned int TARGET_FUNCTION_ARG_BOUNDARY (machine_mode mode, const_tree type)

  This hook returns the alignment boundary, in bits, of an argument with the specified mode and type. The default hook returns `PARM_BOUNDARY` for all arguments.

Target Hook: unsigned int TARGET_FUNCTION_ARG_ROUND_BOUNDARY (machine_mode mode, const_tree type)

  Normally, the size of an argument is rounded up to `PARM_BOUNDARY`, which is the default value for this hook. You can define this hook to return a different value if an argument size must be rounded to a larger value.

Macro: FUNCTION_ARG_REGNO_P (regno)

  A C expression that is nonzero if regno is the number of a hard register in which function arguments are sometimes passed. This does not include implicit arguments such as the static chain and the structure-value address. On many machines, no registers can be used for this purpose since all function arguments are pushed on the stack.

Target Hook: bool TARGET_SPLIT_COMPLEX_ARG (const_tree type)

  This hook should return true if parameter of type type are passed as two scalar parameters. By default, GCC will attempt to pack complex arguments into the target’s word size. Some ABIs require complex arguments to be split and treated as their individual components. For example, on AIX64, complex floats should be passed in a pair of floating point registers, even though a complex float would fit in one 64-bit floating point register.

  The default value of this hook is `NULL`, which is treated as always false.

Target Hook: tree TARGET_BUILD_BUILTIN_VA_LIST (void)

  This hook returns a type node for `va_list` for the target. The default version of the hook returns `void*`.

Target Hook: int TARGET_ENUM_VA_LIST_P (int idx, const char **pname, tree *ptree)

  This target hook is used in function `c_common_nodes_and_builtins` to iterate through the target specific builtin types for va_list. The variable idx is used as iterator. pname has to be a pointer to a `const char *` and ptree a pointer to a `tree` typed variable. The arguments pname and ptree are used to store the result of this macro and are set to the name of the va_list builtin type and its internal type. If the return value of this macro is zero, then there is no more element. Otherwise the IDX should be increased for the next call of this macro to iterate through all types.

Target Hook: tree TARGET_FN_ABI_VA_LIST (tree fndecl)

  This hook returns the va_list type of the calling convention specified by fndecl. The default version of this hook returns `va_list_type_node`.

Target Hook: tree TARGET_CANONICAL_VA_LIST_TYPE (tree type)

  This hook returns the va_list type of the calling convention specified by the type of type. If type is not a valid va_list type, it returns `NULL_TREE`.

Target Hook: tree TARGET_GIMPLIFY_VA_ARG_EXPR (tree valist, tree type, gimple_seq *pre_p, gimple_seq *post_p)

  This hook performs target-specific gimplification of `VA_ARG_EXPR`. The first two parameters correspond to the arguments to `va_arg`; the latter two are as in `gimplify.c:gimplify_expr`.

Target Hook: bool TARGET_VALID_POINTER_MODE (scalar_int_mode mode)

  Define this to return nonzero if the port can handle pointers with machine mode mode. The default version of this hook returns true for both `ptr_mode` and `Pmode`.

Target Hook: bool TARGET_REF_MAY_ALIAS_ERRNO (ao_ref *ref)

  Define this to return nonzero if the memory reference ref may alias with the system C library errno location. The default version of this hook assumes the system C library errno location is either a declaration of type int or accessed by dereferencing a pointer to int.

Target Hook: machine_mode TARGET_TRANSLATE_MODE_ATTRIBUTE (machine_mode mode)

  Define this hook if during mode attribute processing, the port should translate machine_mode mode to another mode. For example, rs6000’s `KFmode`, when it is the same as `TFmode`.

  The default version of the hook returns that mode that was passed in.

Target Hook: bool TARGET_SCALAR_MODE_SUPPORTED_P (scalar_mode mode)

  Define this to return nonzero if the port is prepared to handle insns involving scalar mode mode. For a scalar mode to be considered supported, all the basic arithmetic and comparisons must work.

  The default version of this hook returns true for any mode required to handle the basic C types (as defined by the port). Included here are the double-word arithmetic supported by the code in `optabs.c`.

Target Hook: bool TARGET_VECTOR_MODE_SUPPORTED_P (machine_mode mode)

  Define this to return nonzero if the port is prepared to handle insns involving vector mode mode. At the very least, it must have move patterns for this mode.

Target Hook: bool TARGET_COMPATIBLE_VECTOR_TYPES_P (const_tree type1, const_tree type2)

  Return true if there is no target-specific reason for treating vector types type1 and type2 as distinct types. The caller has already checked for target-independent reasons, meaning that the types are known to have the same mode, to have the same number of elements, and to have what the caller considers to be compatible element types.

  The main reason for defining this hook is to reject pairs of types that are handled differently by the target’s calling convention. For example, when a new N-bit vector architecture is added to a target, the target may want to handle normal N-bit `VECTOR_TYPE` arguments and return values in the same way as before, to maintain backwards compatibility. However, it may also provide new, architecture-specific `VECTOR_TYPE`s that are passed and returned in a more efficient way. It is then important to maintain a distinction between the “normal” `VECTOR_TYPE`s and the new architecture-specific ones.

  The default implementation returns true, which is correct for most targets.

Target Hook: opt_machine_mode TARGET_ARRAY_MODE (machine_mode mode, unsigned HOST_WIDE_INT nelems)

  Return the mode that GCC should use for an array that has nelems elements, with each element having mode mode. Return no mode if the target has no special requirements. In the latter case, GCC looks for an integer mode of the appropriate size if available and uses BLKmode otherwise. Usually the search for the integer mode is limited to `MAX_FIXED_MODE_SIZE`, but the `TARGET_ARRAY_MODE_SUPPORTED_P` hook allows a larger mode to be used in specific cases.

  The main use of this hook is to specify that an array of vectors should also have a vector mode. The default implementation returns no mode.

Target Hook: bool TARGET_ARRAY_MODE_SUPPORTED_P (machine_mode mode, unsigned HOST_WIDE_INT nelems)

  Return true if GCC should try to use a scalar mode to store an array of nelems elements, given that each element has mode mode. Returning true here overrides the usual `MAX_FIXED_MODE` limit and allows GCC to use any defined integer mode.

  One use of this hook is to support vector load and store operations that operate on several homogeneous vectors. For example, ARM NEON has operations like:

      int8x8x3_t vld3_s8 (const int8_t *)

  where the return type is defined as:

      typedef struct int8x8x3_t
      {
        int8x8_t val[3];
      } int8x8x3_t;

  If this hook allows `val` to have a scalar mode, then `int8x8x3_t` can have the same mode. GCC can then store `int8x8x3_t`s in registers rather than forcing them onto the stack.

Target Hook: bool TARGET_LIBGCC_FLOATING_MODE_SUPPORTED_P (scalar_float_mode mode)

  Define this to return nonzero if libgcc provides support for the floating-point mode mode, which is known to pass `TARGET_SCALAR_MODE_SUPPORTED_P`. The default version of this hook returns true for all of `SFmode`, `DFmode`, `XFmode` and `TFmode`, if such modes exist.

Target Hook: opt_scalar_float_mode TARGET_FLOATN_MODE (int n, bool extended)

  Define this to return the machine mode to use for the type `_Floatn`, if extended is false, or the type `_Floatnx`, if extended is true. If such a type is not supported, return `opt_scalar_float_mode ()`. The default version of this hook returns `SFmode` for `_Float32`, `DFmode` for `_Float64` and `_Float32x` and `TFmode` for `_Float128`, if those modes exist and satisfy the requirements for those types and pass `TARGET_SCALAR_MODE_SUPPORTED_P` and `TARGET_LIBGCC_FLOATING_MODE_SUPPORTED_P`; for `_Float64x`, it returns the first of `XFmode` and `TFmode` that exists and satisfies the same requirements; for other types, it returns `opt_scalar_float_mode ()`. The hook is only called for values of n and extended that are valid according to ISO/IEC TS 18661-3:2015; that is, n is one of 32, 64, 128, or, if extended is false, 16 or greater than 128 and a multiple of 32.

Target Hook: bool TARGET_FLOATN_BUILTIN_P (int func)

  Define this to return true if the `_Floatn` and `_Floatnx` built-in functions should implicitly enable the built-in function without the `__builtin_` prefix in addition to the normal built-in function with the `__builtin_` prefix. The default is to only enable built-in functions without the `__builtin_` prefix for the GNU C langauge. In strict ANSI/ISO mode, the built-in function without the `__builtin_` prefix is not enabled. The argument `FUNC` is the `enum built_in_function` id of the function to be enabled.

Target Hook: bool TARGET_SMALL_REGISTER_CLASSES_FOR_MODE_P (machine_mode mode)

  Define this to return nonzero for machine modes for which the port has small register classes. If this target hook returns nonzero for a given mode, the compiler will try to minimize the lifetime of registers in mode. The hook may be called with `VOIDmode` as argument. In this case, the hook is expected to return nonzero if it returns nonzero for any mode.

  On some machines, it is risky to let hard registers live across arbitrary insns. Typically, these machines have instructions that require values to be in specific registers (like an accumulator), and reload will fail if the required hard register is used for another purpose across such an insn.

  Passes before reload do not know which hard registers will be used in an instruction, but the machine modes of the registers set or used in the instruction are already known. And for some machines, register classes are small for, say, integer registers but not for floating point registers. For example, the AMD x86-64 architecture requires specific registers for the legacy x86 integer instructions, but there are many SSE registers for floating point operations. On such targets, a good strategy may be to return nonzero from this hook for `INTEGRAL_MODE_P` machine modes but zero for the SSE register classes.

  The default version of this hook returns false for any mode. It is always safe to redefine this hook to return with a nonzero value. But if you unnecessarily define it, you will reduce the amount of optimizations that can be performed in some cases. If you do not define this hook to return a nonzero value when it is required, the compiler will run out of spill registers and print a fatal error message.

Next: Scalar Return, Previous: Stack Arguments, Up: Stack and Calling [Contents][Index]