Previous: IA-64-Bits, Up: IA-64 Syntax [Contents][Index]

#### 9.17.2.4 Relocations

In addition to the standard IA-64 relocations, the following relocations are implemented by `as`:

`@slotcount(V)`

  Convert the address offset V into a slot count. This pseudo function is available only on VMS. The expression V must be known at assembly time: it can’t reference undefined symbols or symbols in different sections.