Next: NDS32-Regs, Up: NDS32 Syntax [Contents][Index]

#### 9.30.2.1 Special Characters

Use ‘`#`’ at column 1 and ‘`!`’ anywhere in the line except inside quotes.

Multiple instructions in a line are allowed though not recommended and should be separated by ‘`;`’.

Assembler is not case-sensitive in general except user defined label. For example, ‘`jral F1`’ is different from ‘`jral f1`’ while it is the same as ‘`JRAL F1`’.