Next: RISC-V Options, Previous: PowerPC Options, Up: Submodel Options [Contents][Index]

#### 3.19.41 PRU Options

These command-line options are defined for PRU target:

`-minrt`

  Link with a minimum runtime environment, with no support for static initializers and constructors. Using this option can significantly reduce the size of the final ELF binary. Beware that the compiler could still generate code with static initializers and constructors. It is up to the programmer to ensure that the source program will not use those features.

`-mmcu=mcu`

  Specify the PRU MCU variant to use. Check Newlib for the exact list of supported MCUs.

`-mno-relax`

  Make GCC pass the `--no-relax` command-line option to the linker instead of the `--relax` option.

`-mloop`

  Allow (or do not allow) GCC to use the LOOP instruction.

`-mabi=variant`

  Specify the ABI variant to output code for. `-mabi=ti` selects the unmodified TI ABI while `-mabi=gnu` selects a GNU variant that copes more naturally with certain GCC assumptions. These are the differences:

  ‘`Function Pointer Size`’

    TI ABI specifies that function (code) pointers are 16-bit, whereas GNU supports only 32-bit data and code pointers.

  ‘`Optional Return Value Pointer`’

    Function return values larger than 64 bits are passed by using a hidden pointer as the first argument of the function. TI ABI, though, mandates that the pointer can be NULL in case the caller is not using the returned value. GNU always passes and expects a valid return value pointer.

  The current `-mabi=ti` implementation simply raises a compile error when any of the above code constructs is detected. As a consequence the standard C library cannot be built and it is omitted when linking with `-mabi=ti`.

  Relaxation is a GNU feature and for safety reasons is disabled when using `-mabi=ti`. The TI toolchain does not emit relocations for QBBx instructions, so the GNU linker cannot adjust them when shortening adjacent LDI32 pseudo instructions.

Next: RISC-V Options, Previous: PowerPC Options, Up: Submodel Options [Contents][Index]